Static Call Graph - [STM32F103C8x\STM32F103C8x.axf]

# Static Call Graph for image STM32F103C8x\STM32F103C8x.axf

#<CALLGRAPH># ARM Linker, 5060528: Last Updated: Tue May 22 10:15:57 2018

### Maximum Stack Usage = 1920 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ gizwitsHandle ⇒ gizProtocolIssuedDataAck ⇒ uartWrite ⇒ __2printf

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- rbWrite ⇒ rbWrite
- UsageFault_Handler ⇒ UsageFault_Handler
- rbRead ⇒ rbRead

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - BusFault_Handler from stm32f1xx_it.o(i.BusFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DebugMon_Handler from stm32f1xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f103xb.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - HardFault_Handler from stm32f1xx_it.o(i.HardFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - MemManage_Handler from stm32f1xx_it.o(i.MemManage_Handler) referenced from startup_stm32f103xb.o(RESET)
  - NMI_Handler from stm32f1xx_it.o(i.NMI_Handler) referenced from startup_stm32f103xb.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PendSV_Handler from stm32f1xx_it.o(i.PendSV_Handler) referenced from startup_stm32f103xb.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - Reset_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SVC_Handler from stm32f1xx_it.o(i.SVC_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xb.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM2_IRQHandler from stm32f1xx_it.o(i.TIM2_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UART_DMAAbortOnError from stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - USART1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART2_IRQHandler from stm32f1xx_it.o(i.USART2_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UsageFault_Handler from stm32f1xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f103xb.o(.text)
  - fputc from gizwits_product.o(i.fputc) referenced from printf8.o(i.__0printf$8)
  - key1LongPress from main.o(i.key1LongPress) referenced from main.o(i.keyInit)
  - key1ShortPress from main.o(i.key1ShortPress) referenced from main.o(i.keyInit)
  - key2LongPress from main.o(i.key2LongPress) referenced from main.o(i.keyInit)
  - key2ShortPress from main.o(i.key2ShortPress) referenced from main.o(i.keyInit)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> HAL_FLASH_Program
  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> wFlashData
  - >> rbWrite
  - >> rbRead
  - >> gizStandardDecompressionValue
  - >> Pro_W2D_UpdateDataHandle
  - >> Pro_W2D_UpdateCmdHandle
  - >> Pro_D2W_UpdateReady
  - >> gizReportData
  - >> gizProtocolWaitAck
  - >> gizProtocolIssuedProcess
  - >> gizProtocolIssuedDataAck
  - >> gizProtocolGetOnePacket
  - >> gizProtocolGetDeviceInfo
  - >> gizDevReportPolicy
  - >> GAgent_MD5Update
  - >> keyInitOne
  - >> gizwitsHandle
  - >> keyInit

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> gizProtocolGetDeviceInfo
  - >> keyInit

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> wFlashData
  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> gizProtocolWaitAckCheck
  - >> gizProtocolWaitAck
  - >> gizProtocolIssuedProcess
  - >> gizProtocolAckHandle
  - >> userInit
  - >> gizwitsHandle

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> Pro_W2D_UpdateDataHandle
  - >> Pro_D2W_UpdateReady
  - >> gizwitsInit

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> Pro_W2D_UpdateDataHandle

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  FLASH_PageErase (Thumb, 28 bytes, Stack size 0 bytes, stm32f1xx_hal_flash_ex.o(i.FLASH_PageErase))
  [Called By]

  - >> HAL_FLASHEx_Erase

  FLASH_WaitForLastOperation (Thumb, 80 bytes, Stack size 16 bytes, stm32f1xx_hal_flash.o(i.FLASH_WaitForLastOperation))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLASH_WaitForLastOperation
  [Calls]
  - >> HAL_GetTick
  - >> FLASH_SetErrorCode
  [Called By]
  - >> HAL_FLASH_Program
  - >> HAL_FLASHEx_Erase

  GAgent_MD5Decode (Thumb, 32 bytes, Stack size 16 bytes, gagent_md5.o(i.GAgent_MD5Decode))
  [Stack]

  - Max Depth = 16
  - Call Chain = GAgent_MD5Decode
  [Called By]
  - >> GAgent_MD5Transform

  GAgent_MD5Encode (Thumb, 50 bytes, Stack size 16 bytes, gagent_md5.o(i.GAgent_MD5Encode))
  [Stack]

  - Max Depth = 16
  - Call Chain = GAgent_MD5Encode
  [Called By]
  - >> GAgent_MD5Final

  GAgent_MD5Final (Thumb, 70 bytes, Stack size 24 bytes, gagent_md5.o(i.GAgent_MD5Final))
  [Stack]

  - Max Depth = 352
  - Call Chain = GAgent_MD5Final ⇒ GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> GAgent_MD5Update
  - >> GAgent_MD5Encode
  [Called By]
  - >> Pro_W2D_UpdateDataHandle

  GAgent_MD5Init (Thumb, 28 bytes, Stack size 0 bytes, gagent_md5.o(i.GAgent_MD5Init))
  [Called By]

  - >> Pro_W2D_UpdateCmdHandle

  GAgent_MD5Transform (Thumb, 1646 bytes, Stack size 280 bytes, gagent_md5.o(i.GAgent_MD5Transform))
  [Stack]

  - Max Depth = 296
  - Call Chain = GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> GAgent_MD5Decode
  [Called By]
  - >> GAgent_MD5Update

  GAgent_MD5Update (Thumb, 118 bytes, Stack size 32 bytes, gagent_md5.o(i.GAgent_MD5Update))
  [Stack]

  - Max Depth = 328
  - Call Chain = GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> GAgent_MD5Transform
  - >> __aeabi_memcpy
  [Called By]
  - >> Pro_W2D_UpdateDataHandle
  - >> GAgent_MD5Final

  HAL_DMA_Abort_IT (Thumb, 148 bytes, Stack size 8 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_FLASHEx_Erase (Thumb, 160 bytes, Stack size 32 bytes, stm32f1xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_FLASHEx_Erase ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  - >> FLASH_PageErase
  - >> FLASH_MassErase
  [Called By]
  - >> flash_erase_page

  HAL_FLASH_Lock (Thumb, 14 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_Lock))
  [Called By]

  - >> writeFlash
  - >> flash_erase_page

  HAL_FLASH_Program (Thumb, 120 bytes, Stack size 40 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_Program))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_FLASH_Program ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  - >> FLASH_Program_HalfWord
  - >> __aeabi_llsr
  [Called By]
  - >> writeFlash

  HAL_FLASH_Unlock (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.HAL_FLASH_Unlock))
  [Called By]

  - >> writeFlash
  - >> flash_erase_page

  HAL_GPIO_Init (Thumb, 408 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> rgbLedInit
  - >> rgbKeyGpioInit
  - >> MX_GPIO_Init
  - >> HAL_UART_MspInit

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> getKey

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> ledRgbControl
  - >> send32Zero
  - >> datSend
  - >> clkProduce

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_UART_Transmit
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> FLASH_WaitForLastOperation
  - >> UART_WaitOnFlagUntilTimeout

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_Init ⇒ HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  - >> HAL_InitTick
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 122 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> main

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> main
  - >> SystemClock_Config
  - >> HAL_MspInit
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init
  - >> HAL_MspInit

  HAL_NVIC_SystemReset (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SystemReset))
  [Called By]

  - >> mcuRestart

  HAL_RCC_ClockConfig (Thumb, 322 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 74 bytes, Stack size 28 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 750 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> SystemClock_Config
  - >> HAL_InitTick

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_TIMEx_BreakCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutationCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 80 bytes, Stack size 12 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_Base_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_Base_MspInit (Thumb, 30 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_Base_MspInit
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Start_IT))
  [Called By]

  - >> timerInit

  HAL_TIM_ConfigClockSource (Thumb, 242 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> MX_TIM2_Init

  HAL_TIM_IC_CaptureCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 358 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ keyHandle ⇒ readKeyValue ⇒ getKey
  [Calls]
  - >> HAL_TIM_PeriodElapsedCallback
  - >> HAL_TIMEx_CommutationCallback
  - >> HAL_TIMEx_BreakCallback
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  [Called By]
  - >> TIM2_IRQHandler

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 24 bytes, Stack size 8 bytes, gizwits_product.o(i.HAL_TIM_PeriodElapsedCallback))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_TIM_PeriodElapsedCallback ⇒ keyHandle ⇒ readKeyValue ⇒ getKey
  [Calls]
  - >> keyHandle
  - >> gizTimerMs
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_TriggerCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_TriggerCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_UART_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_ErrorCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 266 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_UART_IRQHandler ⇒ UART_Receive_IT ⇒ HAL_UART_RxCpltCallback ⇒ gizPutData ⇒ rbWrite ⇒ rbWrite (Cycle)
  [Calls]
  - >> HAL_DMA_Abort_IT
  - >> HAL_UART_TxCpltCallback
  - >> HAL_UART_ErrorCallback
  - >> UART_Transmit_IT
  - >> UART_Receive_IT
  - >> UART_EndRxTransfer
  [Called By]
  - >> USART2_IRQHandler

  HAL_UART_Init (Thumb, 98 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> main

  HAL_UART_MspInit (Thumb, 116 bytes, Stack size 40 bytes, stm32f1xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Receive_IT (Thumb, 82 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Receive_IT))
  [Called By]

  - >> HAL_UART_RxCpltCallback
  - >> uartInit

  HAL_UART_RxCpltCallback (Thumb, 34 bytes, Stack size 8 bytes, gizwits_product.o(i.HAL_UART_RxCpltCallback))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_RxCpltCallback ⇒ gizPutData ⇒ rbWrite ⇒ rbWrite (Cycle)
  [Calls]
  - >> gizPutData
  - >> HAL_UART_Receive_IT
  [Called By]
  - >> UART_Receive_IT

  HAL_UART_Transmit (Thumb, 186 bytes, Stack size 32 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> fputc

  HAL_UART_Transmit_IT (Thumb, 62 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Transmit_IT))
  [Called By]

  - >> uartWrite

  HAL_UART_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> HAL_UART_IRQHandler

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  Pro_D2W_Ask_Module_Reboot (Thumb, 88 bytes, Stack size 16 bytes, gizwits_protocol.o(i.Pro_D2W_Ask_Module_Reboot))
  [Stack]

  - Max Depth = 64
  - Call Chain = Pro_D2W_Ask_Module_Reboot ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> gizProtocolWaitAck
  - >> gizProtocolHeadInit
  - >> uartWrite
  - >> __2printf
  [Called By]
  - >> main

  Pro_D2W_UpdateReady (Thumb, 166 bytes, Stack size 128 bytes, gizwits_protocol.o(i.Pro_D2W_UpdateReady))
  [Stack]

  - Max Depth = 176
  - Call Chain = Pro_D2W_UpdateReady ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> uartWrite
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> Pro_W2D_UpdateCmdHandle

  Pro_D2W_UpdateSuspend (Thumb, 88 bytes, Stack size 16 bytes, gizwits_protocol.o(i.Pro_D2W_UpdateSuspend))
  [Stack]

  - Max Depth = 64
  - Call Chain = Pro_D2W_UpdateSuspend ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> gizProtocolWaitAck
  - >> gizProtocolHeadInit
  - >> uartWrite
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  Pro_W2D_UpdateCmdHandle (Thumb, 248 bytes, Stack size 56 bytes, gizwits_protocol.o(i.Pro_W2D_UpdateCmdHandle))
  [Stack]

  - Max Depth = 232
  - Call Chain = Pro_W2D_UpdateCmdHandle ⇒ Pro_D2W_UpdateReady ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> flash_erase
  - >> char2hex
  - >> Pro_D2W_UpdateReady
  - >> GAgent_MD5Init
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  Pro_W2D_UpdateDataHandle (Thumb, 276 bytes, Stack size 296 bytes, gizwits_protocol.o(i.Pro_W2D_UpdateDataHandle))
  [Stack]

  - Max Depth = 648
  - Call Chain = Pro_W2D_UpdateDataHandle ⇒ wFlashData ⇒ writeFlash ⇒ HAL_FLASH_Program ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> wFlashData
  - >> flash_erase
  - >> exchangeBytes
  - >> mcuRestart
  - >> GAgent_MD5Update
  - >> GAgent_MD5Final
  - >> memcmp
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SystemClock_Config (Thumb, 104 bytes, Stack size 72 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 132
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> main

  SystemInit (Thumb, 56 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  TIM2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.TIM2_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = TIM2_IRQHandler ⇒ HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ keyHandle ⇒ readKeyValue ⇒ getKey
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  TIM_Base_SetConfig (Thumb, 94 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  USART2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = USART2_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ UART_Receive_IT ⇒ HAL_UART_RxCpltCallback ⇒ gizPutData ⇒ rbWrite ⇒ rbWrite (Cycle)
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  __0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> Pro_W2D_UpdateDataHandle
  - >> Pro_W2D_UpdateCmdHandle
  - >> Pro_D2W_UpdateSuspend
  - >> Pro_D2W_UpdateReady
  - >> gizReportData
  - >> gizProtocolWaitAckCheck
  - >> gizProtocolWaitAck
  - >> gizProtocolResendData
  - >> gizProtocolNTP
  - >> gizProtocolModuleStatus
  - >> gizProtocolIssuedProcess
  - >> gizProtocolIssuedDataAck
  - >> gizProtocolHeadInit
  - >> gizProtocolGetOnePacket
  - >> gizProtocolGetDeviceInfo
  - >> gizProtocolErrorCmd
  - >> gizProtocolCommonAck
  - >> gizProtocolAckHandle
  - >> gizDevReportPolicy
  - >> gizDataPoints2ReportData
  - >> gizDataPoint2Event
  - >> gizCheckReport
  - >> gizPutData
  - >> uartWrite
  - >> gizwitsEventProcess
  - >> gizwitsSetMode
  - >> gizwitsInit
  - >> gizwitsHandle
  - >> Pro_D2W_Ask_Module_Reboot
  - >> main
  - >> key2ShortPress
  - >> key2LongPress
  - >> key1ShortPress
  - >> key1LongPress

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  char2hex (Thumb, 86 bytes, Stack size 8 bytes, common.o(i.char2hex))
  [Stack]

  - Max Depth = 8
  - Call Chain = char2hex
  [Called By]
  - >> Pro_W2D_UpdateCmdHandle

  clkProduce (Thumb, 44 bytes, Stack size 16 bytes, hal_rgb_led.o(i.clkProduce))
  [Stack]

  - Max Depth = 24
  - Call Chain = clkProduce ⇒ ledDelay
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> ledDelay
  [Called By]
  - >> send32Zero
  - >> datSend

  datSend (Thumb, 50 bytes, Stack size 24 bytes, hal_rgb_led.o(i.datSend))
  [Stack]

  - Max Depth = 48
  - Call Chain = datSend ⇒ clkProduce ⇒ ledDelay
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> clkProduce
  [Called By]
  - >> dataDealWithAndSend

  dataDealWithAndSend (Thumb, 56 bytes, Stack size 8 bytes, hal_rgb_led.o(i.dataDealWithAndSend))
  [Stack]

  - Max Depth = 56
  - Call Chain = dataDealWithAndSend ⇒ datSend ⇒ clkProduce ⇒ ledDelay
  [Calls]
  - >> takeAntiCode
  - >> datSend
  [Called By]
  - >> rgbLedInit
  - >> ledRgbControl

  exchangeBytes (Thumb, 16 bytes, Stack size 0 bytes, common.o(i.exchangeBytes))
  [Called By]

  - >> Pro_W2D_UpdateDataHandle
  - >> Pro_D2W_UpdateSuspend
  - >> gizReportData
  - >> gizProtocolNTP
  - >> gizProtocolModuleStatus
  - >> gizProtocolGetOnePacket
  - >> gizProtocolGetDeviceInfo
  - >> gizProtocolErrorCmd
  - >> gizProtocolCommonAck
  - >> gizwitsSetMode
  - >> Pro_D2W_Ask_Module_Reboot

  exchangeWord (Thumb, 4 bytes, Stack size 0 bytes, common.o(i.exchangeWord))
  [Called By]

  - >> gizProtocolNTP

  flash_erase (Thumb, 48 bytes, Stack size 16 bytes, flash.o(i.flash_erase))
  [Stack]

  - Max Depth = 96
  - Call Chain = flash_erase ⇒ flash_erase_page ⇒ HAL_FLASHEx_Erase ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> flash_erase_page
  [Called By]
  - >> Pro_W2D_UpdateDataHandle
  - >> Pro_W2D_UpdateCmdHandle

  flash_erase_page (Thumb, 44 bytes, Stack size 32 bytes, flash.o(i.flash_erase_page))
  [Stack]

  - Max Depth = 80
  - Call Chain = flash_erase_page ⇒ HAL_FLASHEx_Erase ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> HAL_FLASH_Unlock
  - >> HAL_FLASH_Lock
  - >> HAL_FLASHEx_Erase
  [Called By]
  - >> flash_erase

  fputc (Thumb, 20 bytes, Stack size 16 bytes, gizwits_product.o(i.fputc))
  [Stack]

  - Max Depth = 72
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Address Reference Count : 1]
  - printf8.o(i.__0printf$8)

  getKey (Thumb, 84 bytes, Stack size 32 bytes, hal_key.o(i.getKey))
  [Stack]

  - Max Depth = 32
  - Call Chain = getKey
  [Calls]
  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> readKeyValue

  gizAcrossByteJudge (Thumb, 30 bytes, Stack size 0 bytes, datapointtools.o(i.gizAcrossByteJudge))
  [Called By]

  - >> gizStandardDecompressionValue
  - >> gizStandardCompressValue

  gizByteOrderExchange (Thumb, 36 bytes, Stack size 12 bytes, datapointtools.o(i.gizByteOrderExchange))
  [Stack]

  - Max Depth = 12
  - Call Chain = gizByteOrderExchange
  [Called By]
  - >> gizStandardDecompressionValue
  - >> gizDataPoints2ReportData

  gizGetTimerCount (Thumb, 6 bytes, Stack size 0 bytes, gizwits_product.o(i.gizGetTimerCount))
  [Called By]

  - >> gizProtocolWaitAck
  - >> gizProtocolResendData
  - >> gizProtocolAckHandle
  - >> gizDevReportPolicy
  - >> gizwitsHandle

  gizProtocolSum (Thumb, 36 bytes, Stack size 8 bytes, common.o(i.gizProtocolSum))
  [Stack]

  - Max Depth = 8
  - Call Chain = gizProtocolSum
  [Called By]
  - >> Pro_D2W_UpdateSuspend
  - >> Pro_D2W_UpdateReady
  - >> gizReportData
  - >> gizProtocolIssuedDataAck
  - >> gizProtocolGetOnePacket
  - >> gizProtocolGetDeviceInfo
  - >> gizProtocolErrorCmd
  - >> gizProtocolCommonAck
  - >> gizwitsSetMode
  - >> Pro_D2W_Ask_Module_Reboot

  gizPutData (Thumb, 40 bytes, Stack size 16 bytes, gizwits_protocol.o(i.gizPutData))
  [Stack]

  - Max Depth = 48
  - Call Chain = gizPutData ⇒ rbWrite ⇒ rbWrite (Cycle)
  [Calls]
  - >> rbWrite
  - >> __2printf
  [Called By]
  - >> HAL_UART_RxCpltCallback

  gizStandardCompressValue (Thumb, 80 bytes, Stack size 16 bytes, datapointtools.o(i.gizStandardCompressValue))
  [Stack]

  - Max Depth = 16
  - Call Chain = gizStandardCompressValue
  [Calls]
  - >> gizAcrossByteJudge
  [Called By]
  - >> gizDataPoints2ReportData

  gizStandardDecompressionValue (Thumb, 130 bytes, Stack size 80 bytes, datapointtools.o(i.gizStandardDecompressionValue))
  [Stack]

  - Max Depth = 92
  - Call Chain = gizStandardDecompressionValue ⇒ gizByteOrderExchange
  [Calls]
  - >> gizByteOrderExchange
  - >> gizAcrossByteJudge
  - >> __aeabi_memcpy
  [Called By]
  - >> gizDataPoint2Event

  gizTimerMs (Thumb, 10 bytes, Stack size 0 bytes, gizwits_product.o(i.gizTimerMs))
  [Called By]

  - >> HAL_TIM_PeriodElapsedCallback

  gizX2Y (Thumb, 6 bytes, Stack size 0 bytes, datapointtools.o(i.gizX2Y))
  [Called By]

  - >> gizDataPoint2Event

  gizY2X (Thumb, 8 bytes, Stack size 0 bytes, datapointtools.o(i.gizY2X))
  [Called By]

  - >> gizDataPoints2ReportData

  gizwitsEventProcess (Thumb, 222 bytes, Stack size 40 bytes, gizwits_product.o(i.gizwitsEventProcess))
  [Stack]

  - Max Depth = 112
  - Call Chain = gizwitsEventProcess ⇒ ledRgbControl ⇒ dataDealWithAndSend ⇒ datSend ⇒ clkProduce ⇒ ledDelay
  [Calls]
  - >> ledRgbControl
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizwitsHandle (Thumb, 722 bytes, Stack size 944 bytes, gizwits_protocol.o(i.gizwitsHandle))
  [Stack]

  - Max Depth = 1920
  - Call Chain = gizwitsHandle ⇒ gizProtocolIssuedDataAck ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> Pro_W2D_UpdateDataHandle
  - >> Pro_W2D_UpdateCmdHandle
  - >> Pro_D2W_UpdateSuspend
  - >> gizProtocolWaitAckCheck
  - >> gizProtocolNTP
  - >> gizProtocolModuleStatus
  - >> gizProtocolIssuedProcess
  - >> gizProtocolIssuedDataAck
  - >> gizProtocolGetOnePacket
  - >> gizProtocolGetDeviceInfo
  - >> gizProtocolErrorCmd
  - >> gizProtocolCommonAck
  - >> gizProtocolAckHandle
  - >> gizDevReportPolicy
  - >> mcuRestart
  - >> gizwitsEventProcess
  - >> gizGetTimerCount
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> main

  gizwitsInit (Thumb, 46 bytes, Stack size 8 bytes, gizwits_protocol.o(i.gizwitsInit))
  [Stack]

  - Max Depth = 32
  - Call Chain = gizwitsInit ⇒ __2printf
  [Calls]
  - >> rbCreate
  - >> __aeabi_memclr4
  - >> __2printf
  [Called By]
  - >> main

  gizwitsSetMode (Thumb, 214 bytes, Stack size 48 bytes, gizwits_protocol.o(i.gizwitsSetMode))
  [Stack]

  - Max Depth = 96
  - Call Chain = gizwitsSetMode ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> gizProtocolWaitAck
  - >> gizProtocolHeadInit
  - >> uartWrite
  - >> __2printf
  [Called By]
  - >> key2ShortPress
  - >> key2LongPress
  - >> key1ShortPress
  - >> key1LongPress

  key1LongPress (Thumb, 18 bytes, Stack size 8 bytes, main.o(i.key1LongPress))
  [Stack]

  - Max Depth = 104
  - Call Chain = key1LongPress ⇒ gizwitsSetMode ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizwitsSetMode
  - >> __2printf
  [Address Reference Count : 1]
  - main.o(i.keyInit)

  key1ShortPress (Thumb, 18 bytes, Stack size 8 bytes, main.o(i.key1ShortPress))
  [Stack]

  - Max Depth = 104
  - Call Chain = key1ShortPress ⇒ gizwitsSetMode ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizwitsSetMode
  - >> __2printf
  [Address Reference Count : 1]
  - main.o(i.keyInit)

  key2LongPress (Thumb, 28 bytes, Stack size 8 bytes, main.o(i.key2LongPress))
  [Stack]

  - Max Depth = 104
  - Call Chain = key2LongPress ⇒ gizwitsSetMode ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> ledRgbControl
  - >> gizwitsSetMode
  - >> __2printf
  [Address Reference Count : 1]
  - main.o(i.keyInit)

  key2ShortPress (Thumb, 28 bytes, Stack size 8 bytes, main.o(i.key2ShortPress))
  [Stack]

  - Max Depth = 104
  - Call Chain = key2ShortPress ⇒ gizwitsSetMode ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> ledRgbControl
  - >> gizwitsSetMode
  - >> __2printf
  [Address Reference Count : 1]
  - main.o(i.keyInit)

  keyHandle (Thumb, 126 bytes, Stack size 24 bytes, hal_key.o(i.keyHandle))
  [Stack]

  - Max Depth = 72
  - Call Chain = keyHandle ⇒ readKeyValue ⇒ getKey
  [Calls]
  - >> readKeyValue
  [Called By]
  - >> HAL_TIM_PeriodElapsedCallback

  keyInit (Thumb, 90 bytes, Stack size 40 bytes, main.o(i.keyInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = keyInit ⇒ keyInitOne
  [Calls]
  - >> keyParaInit
  - >> keyInitOne
  - >> __aeabi_memcpy4
  - >> __aeabi_memcpy
  [Called By]
  - >> main

  keyInitOne (Thumb, 58 bytes, Stack size 40 bytes, hal_key.o(i.keyInitOne))
  [Stack]

  - Max Depth = 40
  - Call Chain = keyInitOne
  [Calls]
  - >> __aeabi_memcpy
  [Called By]
  - >> keyInit

  keyParaInit (Thumb, 20 bytes, Stack size 0 bytes, hal_key.o(i.keyParaInit))
  [Called By]

  - >> keyInit

  ledDelay (Thumb, 16 bytes, Stack size 8 bytes, hal_rgb_led.o(i.ledDelay))
  [Stack]

  - Max Depth = 8
  - Call Chain = ledDelay
  [Called By]
  - >> clkProduce

  ledRgbControl (Thumb, 46 bytes, Stack size 16 bytes, hal_rgb_led.o(i.ledRgbControl))
  [Stack]

  - Max Depth = 72
  - Call Chain = ledRgbControl ⇒ dataDealWithAndSend ⇒ datSend ⇒ clkProduce ⇒ ledDelay
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> send32Zero
  - >> dataDealWithAndSend
  [Called By]
  - >> gizwitsEventProcess
  - >> key2ShortPress
  - >> key2LongPress

  main (Thumb, 168 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 1920
  - Call Chain = main ⇒ gizwitsHandle ⇒ gizProtocolIssuedDataAck ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> userInit
  - >> userHandle
  - >> uartInit
  - >> timerInit
  - >> gizwitsInit
  - >> gizwitsHandle
  - >> Pro_D2W_Ask_Module_Reboot
  - >> HAL_UART_Init
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_Init
  - >> keyInit
  - >> SystemClock_Config
  - >> MX_TIM2_Init
  - >> MX_GPIO_Init
  - >> HAL_NVIC_SetPriority
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  mcuRestart (Thumb, 10 bytes, Stack size 0 bytes, gizwits_product.o(i.mcuRestart))
  [Calls]

  - >> HAL_NVIC_SystemReset
  [Called By]
  - >> Pro_W2D_UpdateDataHandle
  - >> gizwitsHandle

  rbCanRead (Thumb, 50 bytes, Stack size 4 bytes, ringbuffer.o(i.rbCanRead))
  [Stack]

  - Max Depth = 4
  - Call Chain = rbCanRead
  [Calls]
  - >> rbCapacity
  [Called By]
  - >> rbRead
  - >> gizProtocolGetOnePacket
  - >> rbCanWrite

  rbCanWrite (Thumb, 28 bytes, Stack size 4 bytes, ringbuffer.o(i.rbCanWrite))
  [Stack]

  - Max Depth = 8
  - Call Chain = rbCanWrite ⇒ rbCanRead
  [Calls]
  - >> rbCanRead
  - >> rbCapacity
  [Called By]
  - >> rbWrite

  rbCapacity (Thumb, 12 bytes, Stack size 0 bytes, ringbuffer.o(i.rbCapacity))
  [Called By]

  - >> rbWrite
  - >> rbRead
  - >> rbCanRead
  - >> rbCanWrite

  rbCreate (Thumb, 18 bytes, Stack size 0 bytes, ringbuffer.o(i.rbCreate))
  [Called By]

  - >> gizwitsInit

  rbRead (Thumb, 126 bytes, Stack size 24 bytes, ringbuffer.o(i.rbRead))
  [Stack]

  - Max Depth = 28 + In Cycle
  - Call Chain = rbRead ⇒ rbRead (Cycle)
  [Calls]
  - >> rbRead
  - >> rbCanRead
  - >> rbCapacity
  - >> __aeabi_memcpy
  [Called By]
  - >> rbRead
  - >> gizProtocolGetOnePacket

  rbWrite (Thumb, 142 bytes, Stack size 24 bytes, ringbuffer.o(i.rbWrite))
  [Stack]

  - Max Depth = 32 + In Cycle
  - Call Chain = rbWrite ⇒ rbWrite (Cycle)
  [Calls]
  - >> rbWrite
  - >> rbCapacity
  - >> rbCanWrite
  - >> __aeabi_memcpy
  [Called By]
  - >> rbWrite
  - >> gizPutData

  readKeyValue (Thumb, 130 bytes, Stack size 16 bytes, hal_key.o(i.readKeyValue))
  [Stack]

  - Max Depth = 48
  - Call Chain = readKeyValue ⇒ getKey
  [Calls]
  - >> getKey
  [Called By]
  - >> keyHandle

  rgbKeyGpioInit (Thumb, 44 bytes, Stack size 24 bytes, hal_rgb_led.o(i.rgbKeyGpioInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = rgbKeyGpioInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> userInit

  rgbLedInit (Thumb, 72 bytes, Stack size 24 bytes, hal_rgb_led.o(i.rgbLedInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = rgbLedInit ⇒ dataDealWithAndSend ⇒ datSend ⇒ clkProduce ⇒ ledDelay
  [Calls]
  - >> HAL_GPIO_Init
  - >> send32Zero
  - >> dataDealWithAndSend
  [Called By]
  - >> userInit

  send32Zero (Thumb, 30 bytes, Stack size 8 bytes, hal_rgb_led.o(i.send32Zero))
  [Stack]

  - Max Depth = 32
  - Call Chain = send32Zero ⇒ clkProduce ⇒ ledDelay
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> clkProduce
  [Called By]
  - >> rgbLedInit
  - >> ledRgbControl

  takeAntiCode (Thumb, 8 bytes, Stack size 0 bytes, hal_rgb_led.o(i.takeAntiCode))
  [Called By]

  - >> dataDealWithAndSend

  timerInit (Thumb, 6 bytes, Stack size 0 bytes, gizwits_product.o(i.timerInit))
  [Calls]

  - >> HAL_TIM_Base_Start_IT
  [Called By]
  - >> main

  uartInit (Thumb, 10 bytes, Stack size 0 bytes, gizwits_product.o(i.uartInit))
  [Calls]

  - >> HAL_UART_Receive_IT
  [Called By]
  - >> main

  uartWrite (Thumb, 140 bytes, Stack size 24 bytes, gizwits_product.o(i.uartWrite))
  [Stack]

  - Max Depth = 48
  - Call Chain = uartWrite ⇒ __2printf
  [Calls]
  - >> HAL_UART_Transmit_IT
  - >> __2printf
  [Called By]
  - >> Pro_D2W_UpdateSuspend
  - >> Pro_D2W_UpdateReady
  - >> gizReportData
  - >> gizProtocolResendData
  - >> gizProtocolIssuedDataAck
  - >> gizProtocolGetDeviceInfo
  - >> gizProtocolErrorCmd
  - >> gizProtocolCommonAck
  - >> gizwitsSetMode
  - >> Pro_D2W_Ask_Module_Reboot

  userHandle (Thumb, 2 bytes, Stack size 0 bytes, gizwits_product.o(i.userHandle))
  [Called By]

  - >> main

  userInit (Thumb, 22 bytes, Stack size 8 bytes, gizwits_product.o(i.userInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = userInit ⇒ rgbLedInit ⇒ dataDealWithAndSend ⇒ datSend ⇒ clkProduce ⇒ ledDelay
  [Calls]
  - >> rgbLedInit
  - >> rgbKeyGpioInit
  - >> __aeabi_memclr
  [Called By]
  - >> main

  wFlashData (Thumb, 54 bytes, Stack size 272 bytes, flash.o(i.wFlashData))
  [Stack]

  - Max Depth = 352
  - Call Chain = wFlashData ⇒ writeFlash ⇒ HAL_FLASH_Program ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> writeFlash
  - >> __aeabi_memset
  - >> __aeabi_memcpy
  [Called By]
  - >> Pro_W2D_UpdateDataHandle

  writeFlash (Thumb, 68 bytes, Stack size 24 bytes, flash.o(i.writeFlash))
  [Stack]

  - Max Depth = 80
  - Call Chain = writeFlash ⇒ HAL_FLASH_Program ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> HAL_FLASH_Unlock
  - >> HAL_FLASH_Program
  - >> HAL_FLASH_Lock
  [Called By]
  - >> wFlashData

  ### Local Symbols

  MX_GPIO_Init (Thumb, 96 bytes, Stack size 32 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_TIM2_Init (Thumb, 78 bytes, Stack size 32 bytes, main.o(i.MX_TIM2_Init))
  [Stack]

  - Max Depth = 60
  - Call Chain = MX_TIM2_Init ⇒ HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> main

  gizCheckReport (Thumb, 106 bytes, Stack size 16 bytes, gizwits_protocol.o(i.gizCheckReport))
  [Stack]

  - Max Depth = 40
  - Call Chain = gizCheckReport ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> gizDevReportPolicy

  gizDataPoint2Event (Thumb, 174 bytes, Stack size 24 bytes, gizwits_protocol.o(i.gizDataPoint2Event))
  [Stack]

  - Max Depth = 116
  - Call Chain = gizDataPoint2Event ⇒ gizStandardDecompressionValue ⇒ gizByteOrderExchange
  [Calls]
  - >> gizX2Y
  - >> gizStandardDecompressionValue
  - >> __2printf
  [Called By]
  - >> gizProtocolIssuedProcess

  gizDataPoints2ReportData (Thumb, 92 bytes, Stack size 16 bytes, gizwits_protocol.o(i.gizDataPoints2ReportData))
  [Stack]

  - Max Depth = 40
  - Call Chain = gizDataPoints2ReportData ⇒ __2printf
  [Calls]
  - >> gizY2X
  - >> gizStandardCompressValue
  - >> gizByteOrderExchange
  - >> __2printf
  [Called By]
  - >> gizProtocolIssuedProcess
  - >> gizDevReportPolicy

  gizDevReportPolicy (Thumb, 130 bytes, Stack size 24 bytes, gizwits_protocol.o(i.gizDevReportPolicy))
  [Stack]

  - Max Depth = 104
  - Call Chain = gizDevReportPolicy ⇒ gizReportData ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizReportData
  - >> gizDataPoints2ReportData
  - >> gizCheckReport
  - >> gizGetTimerCount
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolAckHandle (Thumb, 84 bytes, Stack size 8 bytes, gizwits_protocol.o(i.gizProtocolAckHandle))
  [Stack]

  - Max Depth = 64
  - Call Chain = gizProtocolAckHandle ⇒ gizProtocolResendData ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolResendData
  - >> gizGetTimerCount
  - >> __aeabi_memclr
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolCommonAck (Thumb, 80 bytes, Stack size 24 bytes, gizwits_protocol.o(i.gizProtocolCommonAck))
  [Stack]

  - Max Depth = 72
  - Call Chain = gizProtocolCommonAck ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> uartWrite
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolErrorCmd (Thumb, 88 bytes, Stack size 24 bytes, gizwits_protocol.o(i.gizProtocolErrorCmd))
  [Stack]

  - Max Depth = 72
  - Call Chain = gizProtocolErrorCmd ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> gizProtocolHeadInit
  - >> uartWrite
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolGetDeviceInfo (Thumb, 180 bytes, Stack size 128 bytes, gizwits_protocol.o(i.gizProtocolGetDeviceInfo))
  [Stack]

  - Max Depth = 176
  - Call Chain = gizProtocolGetDeviceInfo ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> gizProtocolHeadInit
  - >> uartWrite
  - >> __aeabi_memcpy4
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolGetOnePacket (Thumb, 298 bytes, Stack size 40 bytes, gizwits_protocol.o(i.gizProtocolGetOnePacket))
  [Stack]

  - Max Depth = 68
  - Call Chain = gizProtocolGetOnePacket ⇒ rbRead ⇒ rbRead (Cycle)
  [Calls]
  - >> rbRead
  - >> rbCanRead
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolHeadInit (Thumb, 32 bytes, Stack size 8 bytes, gizwits_protocol.o(i.gizProtocolHeadInit))
  [Stack]

  - Max Depth = 32
  - Call Chain = gizProtocolHeadInit ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> Pro_D2W_UpdateSuspend
  - >> gizReportData
  - >> gizProtocolGetDeviceInfo
  - >> gizProtocolErrorCmd
  - >> gizwitsSetMode
  - >> Pro_D2W_Ask_Module_Reboot

  gizProtocolIssuedDataAck (Thumb, 202 bytes, Stack size 928 bytes, gizwits_protocol.o(i.gizProtocolIssuedDataAck))
  [Stack]

  - Max Depth = 976
  - Call Chain = gizProtocolIssuedDataAck ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> uartWrite
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolIssuedProcess (Thumb, 188 bytes, Stack size 40 bytes, gizwits_protocol.o(i.gizProtocolIssuedProcess))
  [Stack]

  - Max Depth = 156
  - Call Chain = gizProtocolIssuedProcess ⇒ gizDataPoint2Event ⇒ gizStandardDecompressionValue ⇒ gizByteOrderExchange
  [Calls]
  - >> gizDataPoints2ReportData
  - >> gizDataPoint2Event
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolModuleStatus (Thumb, 578 bytes, Stack size 24 bytes, gizwits_protocol.o(i.gizProtocolModuleStatus))
  [Stack]

  - Max Depth = 48
  - Call Chain = gizProtocolModuleStatus ⇒ __2printf
  [Calls]
  - >> exchangeBytes
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolNTP (Thumb, 94 bytes, Stack size 8 bytes, gizwits_protocol.o(i.gizProtocolNTP))
  [Stack]

  - Max Depth = 32
  - Call Chain = gizProtocolNTP ⇒ __2printf
  [Calls]
  - >> exchangeWord
  - >> exchangeBytes
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizProtocolResendData (Thumb, 54 bytes, Stack size 8 bytes, gizwits_protocol.o(i.gizProtocolResendData))
  [Stack]

  - Max Depth = 56
  - Call Chain = gizProtocolResendData ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> uartWrite
  - >> gizGetTimerCount
  - >> __2printf
  [Called By]
  - >> gizProtocolAckHandle

  gizProtocolWaitAck (Thumb, 66 bytes, Stack size 16 bytes, gizwits_protocol.o(i.gizProtocolWaitAck))
  [Stack]

  - Max Depth = 40
  - Call Chain = gizProtocolWaitAck ⇒ __2printf
  [Calls]
  - >> gizGetTimerCount
  - >> __aeabi_memclr
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> Pro_D2W_UpdateSuspend
  - >> gizReportData
  - >> gizwitsSetMode
  - >> Pro_D2W_Ask_Module_Reboot

  gizProtocolWaitAckCheck (Thumb, 44 bytes, Stack size 8 bytes, gizwits_protocol.o(i.gizProtocolWaitAckCheck))
  [Stack]

  - Max Depth = 32
  - Call Chain = gizProtocolWaitAckCheck ⇒ __2printf
  [Calls]
  - >> __aeabi_memclr
  - >> __2printf
  [Called By]
  - >> gizwitsHandle

  gizReportData (Thumb, 128 bytes, Stack size 32 bytes, gizwits_protocol.o(i.gizReportData))
  [Stack]

  - Max Depth = 80
  - Call Chain = gizReportData ⇒ uartWrite ⇒ __2printf
  [Calls]
  - >> gizProtocolSum
  - >> exchangeBytes
  - >> gizProtocolWaitAck
  - >> gizProtocolHeadInit
  - >> uartWrite
  - >> __aeabi_memcpy
  - >> __2printf
  [Called By]
  - >> gizDevReportPolicy

  FLASH_MassErase (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_flash_ex.o(i.FLASH_MassErase))
  [Called By]

  - >> HAL_FLASHEx_Erase

  FLASH_Program_HalfWord (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.FLASH_Program_HalfWord))
  [Called By]

  - >> HAL_FLASH_Program

  FLASH_SetErrorCode (Thumb, 84 bytes, Stack size 0 bytes, stm32f1xx_hal_flash.o(i.FLASH_SetErrorCode))
  [Called By]

  - >> FLASH_WaitForLastOperation

  TIM_ETR_SetConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_TI1_ConfigInputStage (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  UART_DMAAbortOnError (Thumb, 16 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DMAAbortOnError
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_EndRxTransfer (Thumb, 28 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_EndRxTransfer))
  [Called By]

  - >> HAL_UART_IRQHandler

  UART_Receive_IT (Thumb, 150 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 64
  - Call Chain = UART_Receive_IT ⇒ HAL_UART_RxCpltCallback ⇒ gizPutData ⇒ rbWrite ⇒ rbWrite (Cycle)
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 364 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_SetConfig
  [Calls]
  - >> HAL_RCC_GetPCLK1Freq
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> HAL_UART_Init

  UART_Transmit_IT (Thumb, 98 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_Transmit_IT))
  [Called By]

  - >> HAL_UART_IRQHandler

  UART_WaitOnFlagUntilTimeout (Thumb, 100 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_UART_Transmit

  _printf_core (Thumb, 996 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0printf$8

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  ### Undefined Global Symbols