Static Call Graph - [.\Obj\Gokit_Bootloader.axf]

# Static Call Graph for image .\Obj\Gokit_Bootloader.axf

#<CALLGRAPH># ARM Linker, 5060528: Last Updated: Mon Dec 25 17:16:55 2017

### Maximum Stack Usage = 908 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ update_new_system ⇒ ROM_MD5_Check ⇒ GAgent_MD5Final ⇒ GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - BusFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - HardFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - MemManage_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - NMI_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PendSV_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - Reset_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SVC_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SysTick_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_md.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_md.o(.text)
  - fputc from main.o(.text) referenced from printf8.o(i.__0printf$8)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  MSR_MSP (Thumb, 6 bytes, Stack size 0 bytes, flash.o(.emb_text))
  [Called By]

  - >> iap_load_app

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(.text)

  SystemCoreClockUpdate (Thumb, 142 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  FLASH_SetLatency (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_HalfCycleAccessCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_PrefetchBufferCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_Unlock (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> writeFlash
  - >> flash_erase_page
  - >> flash_erase

  FLASH_UnlockBank1 (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_Lock (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> writeFlash
  - >> flash_erase_page
  - >> flash_erase

  FLASH_LockBank1 (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetBank1Status (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> FLASH_WaitForLastBank1Operation
  - >> FLASH_WaitForLastOperation

  FLASH_WaitForLastOperation (Thumb, 38 bytes, Stack size 4 bytes, stm32f10x_flash.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_GetBank1Status
  [Called By]
  - >> FLASH_UserOptionByteConfig
  - >> FLASH_ReadOutProtection
  - >> FLASH_EnableWriteProtection
  - >> FLASH_ProgramOptionByteData
  - >> FLASH_ProgramHalfWord
  - >> FLASH_ProgramWord
  - >> FLASH_EraseOptionBytes
  - >> FLASH_EraseAllPages
  - >> FLASH_ErasePage

  FLASH_ErasePage (Thumb, 72 bytes, Stack size 12 bytes, stm32f10x_flash.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLASH_ErasePage ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> flash_erase_page
  - >> flash_erase

  FLASH_EraseAllPages (Thumb, 68 bytes, Stack size 8 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_WaitForLastBank1Operation (Thumb, 38 bytes, Stack size 4 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_GetBank1Status
  [Called By]
  - >> FLASH_EraseAllBank1Pages

  FLASH_EraseAllBank1Pages (Thumb, 68 bytes, Stack size 8 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastBank1Operation

  FLASH_GetReadOutProtectionStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Called By]

  - >> FLASH_EraseOptionBytes

  FLASH_EraseOptionBytes (Thumb, 150 bytes, Stack size 12 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_GetReadOutProtectionStatus
  - >> FLASH_WaitForLastOperation

  FLASH_ProgramWord (Thumb, 102 bytes, Stack size 20 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ProgramHalfWord (Thumb, 60 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = FLASH_ProgramHalfWord ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> writeFlash

  FLASH_ProgramOptionByteData (Thumb, 72 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_EnableWriteProtection (Thumb, 200 bytes, Stack size 28 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ReadOutProtection (Thumb, 156 bytes, Stack size 12 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_UserOptionByteConfig (Thumb, 88 bytes, Stack size 20 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_GetUserOptionByte (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetWriteProtectionOptionByte (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetPrefetchBufferStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> writeFlash
  - >> flash_erase_page
  - >> flash_erase

  FLASH_GetStatus (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> usart1_init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> usart1_init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> usart1_init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> usart1_init

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> usart1_init

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> fputc

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> usart1_init

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClearITPendingBit (Thumb, 52 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  fputc (Thumb, 32 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - printf8.o(i.__0printf$8)

  usart1_init (Thumb, 166 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = usart1_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> USART_ClearFlag
  [Called By]
  - >> main

  mcu_restart (Thumb, 38 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> update_new_system

  ROM_MD5_Check (Thumb, 172 bytes, Stack size 288 bytes, main.o(.text))
  [Stack]

  - Max Depth = 652
  - Call Chain = ROM_MD5_Check ⇒ GAgent_MD5Final ⇒ GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> __2printf
  - >> memcmp
  - >> __aeabi_memclr4
  - >> rFlashData
  - >> GAgent_MD5Update
  - >> GAgent_MD5Init
  - >> GAgent_MD5Final
  [Called By]
  - >> main
  - >> update_new_system

  update_new_system (Thumb, 178 bytes, Stack size 256 bytes, main.o(.text))
  [Stack]

  - Max Depth = 908
  - Call Chain = update_new_system ⇒ ROM_MD5_Check ⇒ GAgent_MD5Final ⇒ GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> __2printf
  - >> __aeabi_memclr4
  - >> wFlashData
  - >> rFlashData
  - >> flash_erase
  - >> ROM_MD5_Check
  - >> mcu_restart
  [Called By]
  - >> main

  main (Thumb, 176 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 908
  - Call Chain = main ⇒ update_new_system ⇒ ROM_MD5_Check ⇒ GAgent_MD5Final ⇒ GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> SystemInit
  - >> __2printf
  - >> __aeabi_memclr4
  - >> rFlashData
  - >> iap_load_app
  - >> flash_erase
  - >> update_new_system
  - >> ROM_MD5_Check
  - >> usart1_init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  GAgent_MD5Init (Thumb, 26 bytes, Stack size 0 bytes, gagent_md5.o(.text))
  [Called By]

  - >> ROM_MD5_Check

  GAgent_MD5Decode (Thumb, 50 bytes, Stack size 16 bytes, gagent_md5.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = GAgent_MD5Decode
  [Called By]
  - >> GAgent_MD5Transform

  GAgent_MD5Transform (Thumb, 1886 bytes, Stack size 284 bytes, gagent_md5.o(.text))
  [Stack]

  - Max Depth = 300
  - Call Chain = GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> GAgent_MD5Decode
  [Called By]
  - >> GAgent_MD5Update

  GAgent_MD5Update (Thumb, 140 bytes, Stack size 32 bytes, gagent_md5.o(.text))
  [Stack]

  - Max Depth = 332
  - Call Chain = GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> __aeabi_memcpy
  - >> GAgent_MD5Transform
  [Called By]
  - >> GAgent_MD5Final
  - >> ROM_MD5_Check

  GAgent_MD5Encode (Thumb, 62 bytes, Stack size 16 bytes, gagent_md5.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = GAgent_MD5Encode
  [Called By]
  - >> GAgent_MD5Final

  GAgent_MD5Final (Thumb, 204 bytes, Stack size 32 bytes, gagent_md5.o(.text))
  [Stack]

  - Max Depth = 364
  - Call Chain = GAgent_MD5Final ⇒ GAgent_MD5Update ⇒ GAgent_MD5Transform ⇒ GAgent_MD5Decode
  [Calls]
  - >> GAgent_MD5Encode
  - >> GAgent_MD5Update
  [Called By]
  - >> ROM_MD5_Check

  flash_erase_page (Thumb, 36 bytes, Stack size 16 bytes, flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_ClearFlag
  - >> FLASH_ErasePage
  - >> FLASH_Lock
  - >> FLASH_Unlock

  flash_erase (Thumb, 90 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = flash_erase ⇒ __2printf
  [Calls]
  - >> FLASH_ClearFlag
  - >> FLASH_ErasePage
  - >> FLASH_Lock
  - >> FLASH_Unlock
  - >> __2printf
  [Called By]
  - >> main
  - >> update_new_system

  writeFlash (Thumb, 82 bytes, Stack size 24 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = writeFlash ⇒ __2printf
  [Calls]
  - >> FLASH_ClearFlag
  - >> FLASH_ProgramHalfWord
  - >> FLASH_Lock
  - >> FLASH_Unlock
  - >> __2printf
  [Called By]
  - >> wFlashData

  readFlash (Thumb, 26 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = readFlash
  [Called By]
  - >> rFlashData

  wFlashData (Thumb, 80 bytes, Stack size 280 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 328
  - Call Chain = wFlashData ⇒ writeFlash ⇒ __2printf
  [Calls]
  - >> __aeabi_memset
  - >> __aeabi_memcpy
  - >> writeFlash
  [Called By]
  - >> update_new_system

  rFlashData (Thumb, 96 bytes, Stack size 280 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 288
  - Call Chain = rFlashData ⇒ readFlash
  [Calls]
  - >> __aeabi_memcpy
  - >> readFlash
  [Called By]
  - >> main
  - >> update_new_system
  - >> ROM_MD5_Check

  iap_load_app (Thumb, 50 bytes, Stack size 8 bytes, flash.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = iap_load_app ⇒ __2printf
  [Calls]
  - >> __2printf
  - >> MSR_MSP
  [Called By]
  - >> main

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> wFlashData
  - >> rFlashData
  - >> GAgent_MD5Update

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr
  - >> wFlashData

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> main
  - >> update_new_system
  - >> ROM_MD5_Check

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> ROM_MD5_Check

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __0printf$8 (Thumb, 22 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0printf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> writeFlash
  - >> iap_load_app
  - >> flash_erase
  - >> main
  - >> update_new_system
  - >> ROM_MD5_Check

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  _printf_core (Thumb, 996 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0printf$8

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  ### Undefined Global Symbols